**MOTORS & HAND CONTROLS**

Our standard adjustable bed motors are suitable for weights up to 18 stone (115 kg)

The heavy duty adjustable bed motor is suitable for users up to 25 stone (159kg)

German-made Okin motors for electric adjustable beds

Whisper quiet

low power in standby

Easy to install, we have a separate ‘adjustable bed motor installation guide’

fits most adjustable bed mechanisms.

If you are buying a new motor as a replacement please check that the distance between your parallel drive bars is 561mm, so the pitch is 581mm.

(has all the same features of the standard motor but with the increased power of 6000 Newtons. It

Remove the slide covers from the top of the motor

Connect the adjustable bed hand control

Locate the motor over the two hooks of the main drive bars on the adjustable bed mechanism

Select the head end of the motor

Give it a good push to ensure the motor clicks into place

Slide the top covers back into place checking they are located correctly

Pass the hand control through the slats in the mid section to complete the installation.

Important: If you are purchasing Motors or Hand controls as an individual product please call to discuss compatibility before Purchase.